# 

# Getting Started

## Finding a location for your photo printer

* Place the photo printer on a flat, clean surface, in a dry location, and out of direct sunlight.
* Allow at least 12 cm clearance from the back of the photo printer. When connecting power or USB cables, keep the cables clean.
* For proper ventilation, make sure the top and back of the photo printer are not blocked.
* Place the photo printer on a flat, clean surface, in a dry location.

## Finding a location for your photo printer

Warning2Note: Use only the AC power adapter included with your photo printer. Other adapters can damage your camera, photo printer, or computer.

## Finding a location for photo printer

To connect and turn on the power, follow these steps:

|  |  |
| --- | --- |
| **Step** | **Note** |
| 1. Connect the AC power cord to the AC power adapter, then to the back of the photo printer. | The AC power cable included with your photo printer may not require assembly, and may be different from the one shown. |
| 1. Plug the AC power cable into a power outlet. | Place the photo printer on a flat, clean surface, in a dry location |
| 1. Press the On / Off button to turn the power on. | The photo printer initializes and the On/Off button glows steady green. |

Finding a location for your photo printer